Metadata

Load Files: one for each scenarios

Default

Default\_LNHR

Carbontax

Carbontax\_LNHR

RPS

RPS\_LNHR

Tabs

OH-Total Load

IL-Total Load

Hourly electric load in GW for state

Note that the categories below cover >95% of electricity demand. There are some small electric loads not included in the categories below.

OH-LDEV

IL-LDEV

Hourly electric load in GW for light duty electric vehicles in state

OH-MDHD

IL-MDHD

Hourly electric load in GW for medium & heavy duty electric vehicles in state

OH-Non-Seasonal

IL-Non-Seasonal

Hourly electric load in GW for non-seasonal applications in state

Non-seasonal applications includes light such as lighting, industrial electricity use, other transportation, etc.

OH-ResAC

IL-ResAC

Hourly electric load in GW for residential air conditioning

OH-ResSPH

IL-ResSPH

Hourly electric load in GW for residential space heating

OH-ComAC

IL-ComAC

Hourly electric load in GW for commercial building air conditioning

OH-ComSPH

IL-ComSPH

Hourly electric load in GW for commercial building space heating